{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Main","Wells","3D Plot"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":92,"n_cols":23,"rows_kept":92,"cut":false,"hidden":false,"merged":[[15,0,35,0],[37,2,37,22]]}
["Construction Dewatering - Unconfined Aquifer"]
["Brigham Young University - CE En 544"]
[]
[]
[]
[]
[]
[]
[]
["k:",5.0000000000000001E-3,"[cm/s]",null,"xmin:",-50,"[m]",null,"Design h:",35,"[m]"]
["k:",{"$f":"B10/100","v":5.0000000000000002E-5},"[m/s]",null,"xmax:",150,"[m]",null,"Max h:",null,"[m]"]
["H:",40,"[m]",null,"ymin:",-50,"[m]",null,"Total Q:",2.5999999999999999E-2,"[m^3/s]"]
["R:",500,"[m]",null,"ymax:",150,"[m]",null,null,{"$f":"totalQ*(3.28^3)*7.48*60","v":411.76338677759992},"[gal/min]"]
[]
[]
["Y",{"$f":"ymin+B72*(ymax-ymin)","v":150}]
[null,140]
[null,130]
[null,120]
[null,110]
[null,100]
[null,90]
[null,80]
[null,70]
[null,60.000000000000014]
[null,50]
[null,40]
[null,29.999999999999801]
[null,19.999999999999801]
[null,9.999999999999801]
[null,-1.9895196601282805E-13]
[null,-10.000000000000199]
[null,-20.000000000000203]
[null,-30.000000000000199]
[null,-40.000000000000199]
[null,-50]
[null,null,{"$f":"xmin+C72*(xmax-xmin)","v":-50},-40,-30,-20,-10,0,10,20,30,40,50,60.000000000000014,70,80,90,100,110,120,130,140,150]
[null,null,"X"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,1,0,0.05,0.1,0.15,0.2,0.25,0.3,0.35,0.4,0.45,0.5,0.55000000000000004,0.6,0.65,0.7,0.75,0.8,0.85,0.9,0.95,1]
[null,0.95]
[null,0.9]
[null,0.85]
[null,0.8]
[null,0.75]
[null,0.7]
[null,0.65]
[null,0.6]
[null,0.55000000000000004]
[null,0.5]
[null,0.45]
[null,0.39999999999999902]
[null,0.34999999999999898]
[null,0.29999999999999899]
[null,0.249999999999999]
[null,0.19999999999999901]
[null,0.149999999999999]
[null,9.9999999999999006E-2]
[null,4.9999999999998997E-2]
[null,0]

{"sheet":"Wells","index":1,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Wells"]
[]
["#","x","y","Q [m^3/s]"]
[1,-1.3677811550151944,78.605297139726162,{"$f":"totalQ/4","v":6.4999999999999997E-3}]
[2,4.5086119554204629,-12.17484470424548,{"$f":"totalQ/4","v":6.4999999999999997E-3}]
[3,46.251266464032426,70.094658841853814,{"$f":"totalQ/4","v":6.4999999999999997E-3}]
[4,92.857142857142861,12.411443711830181,{"$f":"totalQ/4","v":6.4999999999999997E-3}]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]

{"sheet":"3D Plot","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}